Contents

* CCS12.4.0.00007\_linux-x64.tar.gz - Code Composer Studio 12.4.0: <https://www.ti.com/tool/download/CCSTUDIO/12.4.0>
* simplelink\_cc13xx\_cc26xx\_sdk\_7\_10\_01\_24.run (md5:c834ca645bb888f7ea600f6454d64e90) - Linux Installer for SimpleLink CC13XX CC26XX SDK v7.10.01.24: <https://www.ti.com/tool/download/SIMPLELINK-LOWPOWER-F2-SDK/7.10.01.24>
* cc2538-bsl.py - Python script to flash hex files from Linux. See booklet for a step by step guide.
* Lab2-Detecting-Trackers.zip - Code template for Lab 2
* airtag\_scanner\_CC1352P\_7.hex - Firmware for Lab 2
* Lab3-Spoofing-Trackers.zip - Code template for Lab 3
* sniffle.hex - Firmware for Lab1-Sniffing-Connections
* airtag\_spoofer\_CC1352P\_7.hex - Firmware for Lab 3